First install the program setup.exe.

You must run TSA program using administrator privileges (see manual)

**********************************************************************************************
Demo mode:

When you run the TSA program for the first time after installation, it will be in demo mode.

you can open the program window, and you can open the recode file to watch the test result. 
you find the demo recode folder in the REC folder:

cell_3_signal
CW_1MHZ
Limit_line
Zigbee


Copy the folders listed above from CD files into the C:\Users\username\Documents\Triarchy Tech\TSA Spectrum Analyzer\REC

You also can find limit line demo file at REF folder:

Limit_demo-7dBm.xls

Copy this file into the C:\Users\username\Documents\Triarchy Tech\TSA Spectrum Analyzer\REF

You can use it when you want to check the limit line function.

**********************************************************************************************
Full Mode:

If you ordered the TSAxGx USB Min Spectrum Analyzer product, to get it working in full mode, you need to copy the calibration files into the TSA program files:

find amp_ofst.dat and freq_ofst.dat files in [CD drive]\TSA USB mini Spectrum Analyzer CD\SW_file\Calibration_file

Copy amp_ofst.dat and freq_ofst.dat files into  C:\Users\[username]\Documents\Triarchy Tech\TSA Spectrum Analyzer

Select "Move and Replace" option when the prompt appears. amp_ofst.dat and freq_ofst.dat need replace the old demo calibration files.

Then open the TSA using administrator privileges. TSA program will be working in 4G/5G/6G/12G version, based on your calibration file that is included with your 
purchase. you will find that product SN in TSA program will match with SN on the USB dongle. If the two SN are not matching, it means calibration file in the TSA is 
not matching with your hardware USB dongle. 

You need try to contact Triarchy Technologies to find right calibration file. 
the contact email be: support@triarchytech.com
 